# Introduction

This document contains the design specification for The TTD Device.

# Physical **Requirements**

[r1 c-1] TTD shall be a cube with each edge measuring 15 ± 0.25 cm.

[r2 c-2] TTD shall weigh no more than 8 ± 0.5 kg.

[r3 c-3] All edges of TTD shall be broken or beveled so as to not harm the user.

[r4 c-3] No outer surface of TTD shall be no hotter than 45°C when operated at 30°C.